DCN E1300138-v1

To save costs, D1300135 was revised to be made on a milling machine instead of an EDM. Also added 1/4-20 holes to D1300135. Added missing dimension of #6 thru holes.

J. Lewis 22 Feb 2013