Title: PZT Dewhite Interface Board
Drawing Number: D2500196
Revision: 1
Author: Daniel Sigg
Board Size: 8.00" x 1.25"
Layers: 2
Smallest feature: 10mil
Components: top side only

Manufacturing instructions:
- Preferably use 1oz. copper weight
- Board thickness: approximately 62 mils

Assembly instructions:
- None

Layer Stack (top to bottom):
PZTDewhiteInterface.GTL
PZTDewhiteInterface.GBL

Silkscreen (top/bottom):
PZTDewhiteInterface.GTO

Solder Mask (top/bottom):
PZTDewhiteInterface.GTS
PZTDewhiteInterface.GBS

Paste Mask (top/bottom):
PZTDewhiteInterface.GTP

Board Outline:
PZTDewhiteInterface.GM

NC Drill File:
PZTDewhiteInterface.txt

ODB Files:
PZTDewhiteInterface.zip

Pick and Place:
Pick Place for PZTDewhiteInterface.txt
