Title: CHETA PD Interface Board
Drawing Number: D2500307
Revision: 1
Author: Daniel Sigg
Board Size: 6.40" x 2.00"
Layers: 2
Smallest feature: 10 mils
Components: top side only

Manufacturing instructions:
- Preferably use 1oz. copper weight
- Board thickness: approximately 62 mils

Assembly instructions:
- none

Layer Stack (top to bottom):
ChetaPDInterfaceBoard.GTL
ChetaPDInterfaceBoard.GBL

Silkscreen (top/bottom):
ChetaPDInterfaceBoard.GTO

Solder Mask (top/bottom):
ChetaPDInterfaceBoard.GTS
ChetaPDInterfaceBoard.GBS

Paste Mask (top/bottom):
ChetaPDInterfaceBoard.GTP

Board Outline:
ChetaPDInterfaceBoard.GM

Drill File:
ChetaPDInterfaceBoard.txt

Pick and Place:
Pick Place for ChetaPDInterfaceBoard.txt

ODB+ Files:
ChetaPDInterfaceBoard.zip
