Title: Timing Clock
Drawing Number: D2600005
Revision: 1
Author: Daniel Sigg
Board Size: 3.00" x 2.300"
Layers: 6
Smallest feature: 5mil
Components: both sides

Manufacturing instructions:
- Preferably use 1oz. copper weight
- Board thickness: approximately 62 mils

Assembly instructions:
- Solder large plastic capacitors by hand
- P1/40-pin: solder to top when male header, solder to bottom when female socket

Layer Stack (top to bottom):
TimingClock.GTL
TimingClock.GP1
TimingClock.G1
TimingClock.G2
TimingClock.GP2
TimingClock.GBL

Silkscreen (top/bottom):
TimingClock.GTO
TimingClock.GBO

Solder Mask (top/bottom):
TimingClock.GTS
TimingClock.GBS

Paste Mask (top/bottom):
TimingClock.GTP
TimingClock.GBP

Board Outline:
TimingClock.GM

NC Drill File:
TimingClock.txt

Drill File (gerber):
TimingClock.GD1

Pick and Place:
Pick Place for TimingClock.txt

ODB+ Files:
TimingClock.zip
