|  |  |
| --- | --- |
| *Title* | *All Things Picomotor* |
| *Author* | *R. Abbott, Caltech* |
| *Date* | *20 February 2015* |

# Overview

This is a breakdown of all the Picomotor and Mighty Mouse Connector info that, at time of writing, is in my office (211 Downs Lab

## What I have as of 20 February 2015

Table Data List for Picomotors

|  |  |  |
| --- | --- | --- |
| **Quantity** | **Item** | **Notes** |
| 15 | UHV-KAP Picomotor | All in the bags clean with no connectors on wire ends. These are the latest model with nice long wires. |
| 6 | Old model 8301-UHV Picomotor | These were the original units that require wire length extension and connector to be put into service |
| 4 | Old model 8301-UHV Picomotor | These units had wire failure and are in need of repair. They are now mildly dirty which presents a quandary |
| 2 | Old model 8301 Picomotors with attached connector | This bag has a note “with stop nut damaged” and presumably needs repair |
| 2 | Old model 8301 Picomotors with attached connector | This bag has a note “Taken out of TMS, one channel bad, needs inspection” |
| 23 | Male Mighty Mouse connectors and associated pins | All clean ready to crimp onto wires and mount on picomotor bracket. |
| 5 | Female cable end Mighty Mouse connectors for cable ends | All clean and ready to put onto cable harness if needed. |
| 1 | Pin extraction tool | Class A clean and ready to go |